{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet0","index":0,"n_rows":180,"n_cols":19,"rows_kept":180,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["ID","一级","二级","图片路径","型号","PDF","URl","中文名称","特性","长度","端头A","端头B","材质","工作温度°C","电缆类型","手持测试最大电压（CE标准）","电流","离手使用最大电压","颜色"]
["563","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-4-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","4in(0.1m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["564","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-8-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","8in(0.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["565","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-12-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","12in(0.3m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["566","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-18-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","18in(0.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["567","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-24-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","24in(0.6m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["568","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-36-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","36in(0.9m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["569","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-48-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","48in(1.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["570","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-60-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","60in(1.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["571","跳线和测试线","香蕉插头","/跳线和测试线/B.jpg","B-72-*","/跳线和测试线/B.pdf","","多叠接香蕉插头跳线","1.交叉和垂直堆叠；2.快速连接的理想跳线","72in(1.8m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0-9"]
["572","跳线和测试线","香蕉插头","/跳线和测试线/2948.jpg","2948-12-*","/跳线和测试线/2948.pdf","","多叠接香蕉插头跳线","1.标准香蕉插头和插孔；\r\n2.大大简化了电路连接和更改；\r\n3.可靠的焊接连接承受拉力测试超过50磅；\r\n4.垂直和横向可堆叠。","12in(0.3m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀金铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["573","跳线和测试线","香蕉插头","/跳线和测试线/2948.jpg","2948-24-*","/跳线和测试线/2948.pdf","","多叠接香蕉插头跳线","1.标准香蕉插头和插孔；\r\n2.大大简化了电路连接和更改；\r\n3.可靠的焊接连接承受拉力测试超过50磅；\r\n4.垂直和横向可堆叠。","24in(0.6m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀金铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["574","跳线和测试线","香蕉插头","/跳线和测试线/2948.jpg","2948-36-*","/跳线和测试线/2948.pdf","","多叠接香蕉插头跳线","1.标准香蕉插头和插孔；\r\n2.大大简化了电路连接和更改；\r\n3.可靠的焊接连接承受拉力测试超过50磅；\r\n4.垂直和横向可堆叠。","36in(0.9m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀金铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["575","跳线和测试线","香蕉插头","/跳线和测试线/2948.jpg","2948-48-*","/","","多叠接香蕉插头跳线","1.标准香蕉插头和插孔；\r\n2.大大简化了电路连接和更改；\r\n3.可靠的焊接连接承受拉力测试超过50磅；\r\n4.垂直和横向可堆叠。","48in(1.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀金铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["576","跳线和测试线","香蕉插头","/跳线和测试线/2948.jpg","2948-60-*","/跳线和测试线/2948.pdf","","多叠接香蕉插头跳线","1.标准香蕉插头和插孔；\r\n2.大大简化了电路连接和更改；\r\n3.可靠的焊接连接承受拉力测试超过50磅；\r\n4.垂直和横向可堆叠。","60in(1.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀金铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["577","跳线和测试线","香蕉插头","/跳线和测试线/HB.jpg","HB-12-*","/跳线和测试线/HB.pdf","","水平叠接香蕉插头跳线","1.正面和垂直堆叠香蕉插头;\r\n2.与标准香蕉插孔配合;\r\n3.机箱上提供跳线的理想选择；4.接触电阻:小于1mΩ。","12in(0.3m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","33VAC/70VDC","15A","5000V","0、2"]
["578","跳线和测试线","香蕉插头","/跳线和测试线/HB.jpg","HB-24-*","/跳线和测试线/HB.pdf","","水平叠接香蕉插头跳线","1.正面和垂直堆叠香蕉插头;\r\n2.与标准香蕉插孔配合;\r\n3.机箱上提供跳线的理想选择；4.接触电阻:小于1mΩ。","24in(0.6m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","33VAC/70VDC","15A","5000V","0、2"]
["579","跳线和测试线","香蕉插头","/跳线和测试线/HB.jpg","HB-36-*","/跳线和测试线/HB.pdf","","水平叠接香蕉插头跳线","1.正面和垂直堆叠香蕉插头;\r\n2.与标准香蕉插孔配合;\r\n3.机箱上提供跳线的理想选择；4.接触电阻:小于1mΩ。","36in(0.9m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","33VAC/70VDC","15A","5000V","0、2"]
["580","跳线和测试线","香蕉插头","/跳线和测试线/HB.jpg","HB-48-*","/跳线和测试线/HB.pdf","","水平叠接香蕉插头跳线","1.正面和垂直堆叠香蕉插头;\r\n2.与标准香蕉插孔配合;\r\n3.机箱上提供跳线的理想选择；4.接触电阻:小于1mΩ。","48in(1.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","33VAC/70VDC","15A","5000V","0、2"]
["581","跳线和测试线","香蕉插头","/跳线和测试线/HB.jpg","HB-60-*","/跳线和测试线/HB.pdf","","水平叠接香蕉插头跳线","1.正面和垂直堆叠香蕉插头;\r\n2.与标准香蕉插孔配合;\r\n3.机箱上提供跳线的理想选择；4.接触电阻:小于1mΩ。","60in(1.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","33VAC/70VDC","15A","5000V","0、2"]
["582","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-12-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","12in(0.3m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["583","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-18-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","18in(0.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["584","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-24-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","24in(0.6m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["585","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-36-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","36in(0.9m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["586","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-48-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","48in(1.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["587","跳线和测试线","香蕉插头","/跳线和测试线/1440.jpg","1440-60-*","/跳线和测试线/1440.pdf","","交叉叠接香蕉插头跳线","1.交叉堆叠香蕉插头；\r\n2.提供跳线或机箱的理想选择；3.香蕉插头直径5.33mm。","60in(1.5m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["588","跳线和测试线","香蕉插头","/跳线和测试线/6727.jpg","6727-*","/跳线和测试线/6727.pdf","","多叠接护套4mm香蕉插头跳线","1.导线为多股铜线；3.绝缘为硅树脂；4.跳线可以垂直堆叠；\r\n5.符合国际安全标准IEC1010-2-031。","48in(1.2m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","-10℃至+55℃（+14℉至+131℉）","NA","NA","20A","CATⅢ 1000V","0、2"]
["589","跳线和测试线","香蕉插头","/跳线和测试线/3014.jpg","3014-36-*","/跳线和测试线/3014.pdf","","多叠接香蕉插头至小型叠接香蕉插头","1.将标准香蕉插头4.32mm转换为迷你香蕉插头3.05mm，或将迷你香蕉插头转换为标准香蕉插头；\r\n2.交叉和垂直堆叠香蕉插座。","36in(0.9m)","单香蕉插头","小型香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","3000V","0、2"]
["590","跳线和测试线","香蕉插头","/跳线和测试线/3014.jpg","3014-60-*","/跳线和测试线/3014.pdf","","多叠接香蕉插头至小型叠接香蕉插头","1.将标准香蕉插头4.32mm转换为迷你香蕉插头3.05mm，或将迷你香蕉插头转换为标准香蕉插头；\r\n2.交叉和垂直堆叠香蕉插座。","60in(1.5m)","单香蕉插头","小型香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","3000V","0、2"]
["591","跳线和测试线","香蕉插头","/跳线和测试线/6249.jpg","6249-12-*","/跳线和测试线/6249.pdf","","多叠接香蕉插头至Mini测试夹","1.新设计的Minigrabber?测试夹跳线可提供300V电压和5A电流的额定值；\r\n2.抓斗宽度很窄，只有0.36英寸（9.14毫米），可轻松接入测试端子。\r\n3.抓钩是镀金铍铜，以确保信号完整性并附着在组件引线上，外径1.060英寸（1.5毫米）；\r\n4.采集器跳线直接连接到配置为非护套式设备；\r\n5.插头采用一体式整体设计直接模制到电缆上，可实现持久的连接；\r\n6.多叶香蕉弹簧材料为镀镍铍铜，可延长插入寿命并降低接触抵抗性；\r\n7.香蕉插头具有顶部和侧面堆叠的功能，从而增加了测试的多功能性；\r\n8.高股数硅胶绝","12in(0.3m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","NA","18AWG","30VAC/60VDC","5A","300V","0、2"]
["592","跳线和测试线","香蕉插头","/跳线和测试线/6249.jpg","6249-24-*","/跳线和测试线/6249.pdf","","多叠接香蕉插头至Mini测试夹","1.新设计的Minigrabber?测试夹跳线可提供300V电压和5A电流的额定值；\r\n2.抓斗宽度很窄，只有0.36英寸（9.14毫米），可轻松接入测试端子。\r\n3.抓钩是镀金铍铜，以确保信号完整性并附着在组件引线上，外径1.060英寸（1.5毫米）；\r\n4.采集器跳线直接连接到配置为非护套式设备；\r\n5.插头采用一体式整体设计直接模制到电缆上，可实现持久的连接；\r\n6.多叶香蕉弹簧材料为镀镍铍铜，可延长插入寿命并降低接触抵抗性；\r\n7.香蕉插头具有顶部和侧面堆叠的功能，从而增加了测试的多功能性；\r\n8.高股数硅胶绝","24in(0.6m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","NA","18AWG","30VAC/60VDC","5A","300V","0、2"]
["593","跳线和测试线","香蕉插头","/跳线和测试线/6249.jpg","6249-36-*","/跳线和测试线/6249.pdf","","多叠接香蕉插头至Mini测试夹","1.新设计的Minigrabber?测试夹跳线可提供300V电压和5A电流的额定值；\r\n2.抓斗宽度很窄，只有0.36英寸（9.14毫米），可轻松接入测试端子。\r\n3.抓钩是镀金铍铜，以确保信号完整性并附着在组件引线上，外径1.060英寸（1.5毫米）；\r\n4.采集器跳线直接连接到配置为非护套式设备；\r\n5.插头采用一体式整体设计直接模制到电缆上，可实现持久的连接；\r\n6.多叶香蕉弹簧材料为镀镍铍铜，可延长插入寿命并降低接触抵抗性；\r\n7.香蕉插头具有顶部和侧面堆叠的功能，从而增加了测试的多功能性；\r\n8.高股数硅胶绝","36in(0.9m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","NA","18AWG","30VAC/60VDC","5A","300V","0、2"]
["594","跳线和测试线","香蕉插头","/跳线和测试线/3782.jpg","3782-12-*","/跳线和测试线/3782.pdf","","多叠接香蕉插头至Mini测试夹","1.提供来自香蕉插孔的Minigrabbe测试夹r输出；\r\n2.香蕉插头可以垂直和交叉堆叠。","12in(0.3m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2、4、5、6"]
["595","跳线和测试线","香蕉插头","/跳线和测试线/3782.jpg","3782-24-*","/跳线和测试线/3782.pdf","","多叠接香蕉插头至Mini测试夹","1.提供来自香蕉插孔的Minigrabbe测试夹r输出；\r\n2.香蕉插头可以垂直和交叉堆叠。","24in(0.6m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2、4、5、6"]
["596","跳线和测试线","香蕉插头","/跳线和测试线/3782.jpg","3782-36-*","/跳线和测试线/3782.pdf","","多叠接香蕉插头至Mini测试夹","1.提供来自香蕉插孔的Minigrabbe测试夹r输出；\r\n2.香蕉插头可以垂直和交叉堆叠。","36in(0.9m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2、4、5、6"]
["597","跳线和测试线","香蕉插头","/跳线和测试线/3782.jpg","3782-48-*","/跳线和测试线/3782.pdf","","多叠接香蕉插头至Mini测试夹","1.提供来自香蕉插孔的Minigrabbe测试夹r输出；\r\n2.香蕉插头可以垂直和交叉堆叠。","48in(1.2m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2、4、5、6"]
["598","跳线和测试线","香蕉插头","/跳线和测试线/3782.jpg","3782-60-*","/跳线和测试线/3782.pdf","","多叠接香蕉插头至Mini测试夹","1.提供来自香蕉插孔的Minigrabbe测试夹r输出；\r\n2.香蕉插头可以垂直和交叉堆叠。","60in(1.5m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2、4、5、6"]
["599","跳线和测试线","香蕉插头","/跳线和测试线/2864.jpg","2864-24-*","/跳线和测试线/2864.pdf","","直角叠接香蕉插头跳线","1.垂直堆叠功能可实现连续的电路连接，并且直角设计可使电线靠近机箱；\r\n2.线长可以轻松连接和断开连接。","24in(0.6m)","单香蕉插头","单香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["600","跳线和测试线","香蕉插头","/跳线和测试线/6248.jpg","6248-12-*","/跳线和测试线/6248.pdf","","Mini测试夹带护套","1.新设计的Minigrabber?测试夹跳线符合IEC61010-2-31，这是测试配件的最新国际安全标准；\r\n2.抓斗宽度很窄，只有0.36英寸（9.14毫米），可轻松接入测试端子；\r\n3.抓钩是镀金铍铜，以确保信号完整性，并附着在外径达0.060英寸（1.5毫米）的组件引线上；\r\n4.抓斗跳线可以直接连接至Pomona的护套型柔性测试线，以增加跳线的长度；\r\n5.香蕉插孔直接模制到电缆上，以实现持久连接；\r\n6.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","12in(0.3m)","单香蕉插孔","单迷你测试夹","主体：镀镍黄铜；挂钩：镀金铍铜","NA","18AWG","NA","5A","CATⅡ 300V","0、2"]
["601","跳线和测试线","香蕉插头","/跳线和测试线/5053.jpg","5053-24-*","/跳线和测试线/5053.pdf","","多叠接香蕉插头至微型测试夹","1.香蕉插头可横向堆叠和垂直堆叠；\r\n2.非常适合将测试设备连接到小型电路板组件。","24in(0.6m)","单香蕉插头","单微型测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","3A","150V","0、2"]
["602","跳线和测试线","香蕉插头","/跳线和测试线/5053.jpg","5053-36-*","/跳线和测试线/5053.pdf","","多叠接香蕉插头至微型测试夹","1.香蕉插头可横向堆叠和垂直堆叠；\r\n2.非常适合将测试设备连接到小型电路板组件。","36in(0.9m)","单香蕉插头","单微型测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","3A","150V","0、2"]
["603","跳线和测试线","香蕉插头","/跳线和测试线/5053.jpg","5053-48-*","/跳线和测试线/5053.pdf","","多叠接香蕉插头至微型测试夹","1.香蕉插头可横向堆叠和垂直堆叠；\r\n2.非常适合将测试设备连接到小型电路板组件。","48in(1.2m)","单香蕉插头","单微型测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","3A","150V","0、2"]
["604","跳线和测试线","香蕉插头","/跳线和测试线/6244.jpg","6244-48-*","/跳线和测试线/6244.pdf","","Mini测试夹测试线","1.直角DMM；2.新设计的Minigrabber?测试夹跳线符合最新国际安全标准IEC 61010-2-31；\r\n3.抓斗宽度很窄，只有0.36英寸（9.14毫米），可以轻松并排堆叠；\r\n4.抓钩是镀金铍铜，以确保信号完整性，并附着在外径达0.060英寸（1.5毫米）的组件引线上；\r\n5.采集器跳线直接连接到配置了4毫米护套安全插孔的设备；\r\n6.插头以一体式整体设计直接模制到电缆上，并且电线被双重压接，以实现持久的连接；\r\n7.多叶香蕉弹簧材料是镀镍铍铜，可延长插入寿命并降低接触电阻；\r\n8.高股数硅胶绝缘电线具","48in(1.2m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","NA","18AWG","NA","5A","CATⅡ 300V","0、2"]
["605","跳线和测试线","香蕉插头","/跳线和测试线/6245.jpg","6245-48-*","/跳线和测试线/6245.pdf","","Mini测试夹测试线","1.直插式DMM；2.新设计的Minigrabber?测试夹跳线符合最新国际安全标准IEC 61010-2-31；\r\n2.抓斗宽度很窄，只有0.36英寸（9.14毫米），可以轻松并排堆叠；\r\n3.抓钩是镀金铍铜，以确保信号完整性，并附着在外径达0.060英寸（1.5毫米）的组件引线上；\r\n4.采集器跳线直接连接到配置了5毫米护套安全插孔的设备；\r\n5.插头以一体式整体设计直接模制到电缆上，并且电线被双重压接，以实现持久的连接；\r\n6.多叶香蕉弹簧材料是镀镍铍铜，可延长插入寿命并降低接触电阻；\r\n7.高股数硅胶绝缘电线","48in(1.2m)","单香蕉插头","单迷你测试夹","主体：镀镍黄铜；弹簧：镀镍铍铜；挂钩：镀金铍铜","NA","18AWG","NA","5A","CATⅡ 300V","0、2"]
["606","跳线和测试线","香蕉插头","/跳线和测试线/6283.jpg","6283-C-36","/跳线和测试线/6283.pdf","","双香蕉插头（带安全护套）","1.电缆设计用于所有间距为0.75英寸（19毫米）的标准.166英寸或4mm直径带罩香蕉插座；\r\n2.Pomona的双香蕉插头可用于大多数数字万用表；\r\n3.偏移设计和颜色编码的黑色和红色安全罩消除了错误的极性连接；\r\n4.制造符合最新的安全标准。\r\n5.模制应力消除装置提高了电缆的可靠性和耐用性。","36in(0.9m)","双香蕉插头","双香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","600V","NA"]
["607","跳线和测试线","香蕉插头","/跳线和测试线/6283.jpg","6283-C-48","/跳线和测试线/6283.pdf","","双香蕉插头（带安全护套）","1.电缆设计用于所有间距为0.75英寸（19毫米）的标准.166英寸或4mm直径带罩香蕉插座；\r\n2.Pomona的双香蕉插头可用于大多数数字万用表；\r\n3.偏移设计和颜色编码的黑色和红色安全罩消除了错误的极性连接；\r\n4.制造符合最新的安全标准。\r\n5.模制应力消除装置提高了电缆的可靠性和耐用性。","48in(1.2m)","双香蕉插头","双香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","600V","NA"]
["608","跳线和测试线","香蕉插头","/跳线和测试线/6283.jpg","6283-C-60","/跳线和测试线/6283.pdf","","双香蕉插头（带安全护套）","1.电缆设计用于所有间距为0.75英寸（19毫米）的标准.166英寸或4mm直径带罩香蕉插座；\r\n2.Pomona的双香蕉插头可用于大多数数字万用表；\r\n3.偏移设计和颜色编码的黑色和红色安全罩消除了错误的极性连接；\r\n4.制造符合最新的安全标准。\r\n5.模制应力消除装置提高了电缆的可靠性和耐用性。","60in(1.5m)","双香蕉插头","双香蕉插头","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","600V","NA"]
["609","跳线和测试线","香蕉插头","/跳线和测试线/4768.jpg","4768-k-24","/跳线和测试线/4768.pdf","","双香蕉插头至微型测试夹","1.将双重香蕉插孔转换为微型测试夹；2.叠接\r\n","24in(0.6m)","双香蕉插头","双微型测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","20AWG","NA","NA","1000V","NA"]
["610","跳线和测试线","香蕉插头","/跳线和测试线/4768.jpg","4768-k-36","/跳线和测试线/4768.pdf","","双香蕉插头至微型测试夹","1.将双重香蕉插孔转换为双微型测试夹；2.挂钩为镀金铍铜\r\n","36in(0.9m)","双香蕉插头","双微型测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","20AWG","NA","NA","1000V","NA"]
["611","跳线和测试线","香蕉插头","/跳线和测试线/4768.jpg","4768-k-48","/跳线和测试线/4768.pdf","","双香蕉插头至微型测试夹","1.将双重香蕉插孔转换为双微型测试夹；2.挂钩为镀金铍铜\r\n","48in(1.2m)","双香蕉插头","双微型测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","20AWG","NA","NA","1000V","NA"]
["612","跳线和测试线","香蕉插头","/跳线和测试线/4768.jpg","4768-k-60","/跳线和测试线/4768.pdf","","双香蕉插头至微型测试夹","1.将双重香蕉插孔转换为双微型测试夹；2.挂钩为镀金铍铜\r\n","60in(1.5m)","双香蕉插头","双微型测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","20AWG","NA","NA","1000V","NA"]
["613","跳线和测试线","香蕉插头","/跳线和测试线/1167.jpg","1167-18","/跳线和测试线/1167.pdf","","双导线屏蔽香蕉插头线","1.应用于音频应用，其中低阻抗屏蔽需要平衡线。\r\n2.香蕉插头采用铍铜弹簧，插入寿命长，可水平/垂直堆叠。\r\n3.香蕉插头是模制直接到电缆和电线具有强大的拉力。","18in(0.5m)","双香蕉插头+单屏蔽线","双香蕉插头+单屏蔽线","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","22AWG/屏蔽线:20AWG","33VAC/70VDC","NA","1000V","NA"]
["614","跳线和测试线","香蕉插头","/跳线和测试线/1167.jpg","1167-24","/跳线和测试线/1167.pdf","","双导线屏蔽香蕉插头线","1.应用于音频应用，其中低阻抗屏蔽需要平衡线。\r\n2.香蕉插头采用铍铜弹簧，插入寿命长，可水平/垂直堆叠。\r\n4.香蕉插头是模制直接到电缆和电线具有强大的拉力。","24in(0.6m)","双香蕉插头+单屏蔽线","双香蕉插头+单屏蔽线","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","22AWG/屏蔽线:20AWG","33VAC/70VDC","NA","1000V","NA"]
["615","跳线和测试线","香蕉插头","/跳线和测试线/1167.jpg","1167-36","/跳线和测试线/1167.pdf","","双导线屏蔽香蕉插头线","1.应用于音频应用，其中低阻抗屏蔽需要平衡线。\r\n2.香蕉插头采用铍铜弹簧，插入寿命长，可水平/垂直堆叠。\r\n5.香蕉插头是模制直接到电缆和电线具有强大的拉力。","36in(0.9m)","双香蕉插头+单屏蔽线","双香蕉插头+单屏蔽线","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","22AWG/屏蔽线:20AWG","33VAC/70VDC","NA","1000V","NA"]
["616","跳线和测试线","香蕉插头","/跳线和测试线/1167.jpg","1167-48","/跳线和测试线/1167.pdf","","双导线屏蔽香蕉插头线","1.应用于音频应用，其中低阻抗屏蔽需要平衡线。\r\n2.香蕉插头采用铍铜弹簧，插入寿命长，可水平/垂直堆叠。\r\n6.香蕉插头是模制直接到电缆和电线具有强大的拉力。","48in(1.2m)","双香蕉插头+单屏蔽线","双香蕉插头+单屏蔽线","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","22AWG/屏蔽线:20AWG","33VAC/70VDC","NA","1000V","NA"]
["617","跳线和测试线","香蕉插头","/跳线和测试线/1167.jpg","1167-60","/跳线和测试线/1167.pdf","","双导线屏蔽香蕉插头线","1.应用于音频应用，其中低阻抗屏蔽需要平衡线。\r\n2.香蕉插头采用铍铜弹簧，插入寿命长，可水平/垂直堆叠。\r\n7.香蕉插头是模制直接到电缆和电线具有强大的拉力。","60in(1.5m)","双香蕉插头+单屏蔽线","双香蕉插头+单屏蔽线","主体：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","22AWG/屏蔽线:20AWG","33VAC/70VDC","NA","1000V","NA"]
["618","跳线和测试线","香蕉插头","/跳线和测试线/3786.jpg","3786-c-18","/跳线和测试线/3786.pdf","","多叠接双香蕉插头至迷你测试夹","1.将双重香蕉插孔转换为Minigrabber测试夹；2.叠接\r\n","18in(0.5m)","多叠接双香蕉插头","双迷你测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","NA","5A","300V","NA"]
["619","跳线和测试线","香蕉插头","/跳线和测试线/3786.jpg","3786-c-24","/跳线和测试线/3786.pdf","","多叠接双香蕉插头至迷你测试夹","1.将双重香蕉插孔转换为Minigrabber测试夹；2.叠接\r\n","24in(0.6m)","多叠接双香蕉插头","双迷你测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","NA","5A","300V","NA"]
["620","跳线和测试线","香蕉插头","/跳线和测试线/3786.jpg","3786-c-36","/跳线和测试线/3786.pdf","","多叠接双香蕉插头至迷你测试夹","1.将双重香蕉插孔转换为Minigrabber测试夹；2.叠接\r\n","36in(0.9m)","多叠接双香蕉插头","双迷你测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","NA","5A","300V","NA"]
["621","跳线和测试线","香蕉插头","/跳线和测试线/3786.jpg","3786-c-48","/跳线和测试线/3786.pdf","","多叠接双香蕉插头至迷你测试夹","1.将双重香蕉插孔转换为Minigrabber测试夹；2.叠接\r\n","48in(1.2m)","多叠接双香蕉插头","双迷你测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","NA","5A","300V","NA"]
["622","跳线和测试线","香蕉插头","/跳线和测试线/3786.jpg","3786-c-60","/跳线和测试线/3786.pdf","","多叠接双香蕉插头至迷你测试夹","1.将双重香蕉插孔转换为Minigrabber测试夹；2.叠接\r\n","60in(1.5m)","多叠接双香蕉插头","双迷你测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；测试夹：挂钩：镀金铍铜","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","NA","5A","300V","NA"]
["623","跳线和测试线","香蕉插头","/跳线和测试线/1368.jpg","1368-A-18","/跳线和测试线/1368.pdf","","多叠接双香蕉插头至多叠接香蕉插头","将电源或测试设备连接到面包板的理想选择","18in(0.5m)","多叠接双香蕉插头","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","NA","NA","300V","NA"]
["624","跳线和测试线","香蕉插头","/跳线和测试线/1368.jpg","1368-A-24","/跳线和测试线/1368.pdf","","多叠接双香蕉插头至多叠接香蕉插头","将电源或测试设备连接到面包板的理想选择","24in(0.6m)","多叠接双香蕉插头","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","NA","NA","300V","NA"]
["625","跳线和测试线","香蕉插头","/跳线和测试线/1368.jpg","1368-A-36","/跳线和测试线/1368.pdf","","多叠接双香蕉插头至多叠接香蕉插头","将电源或测试设备连接到面包板的理想选择","36in(0.9m)","多叠接双香蕉插头","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","NA","NA","300V","NA"]
["626","跳线和测试线","香蕉插头","/跳线和测试线/1368.jpg","1368-A-48","/跳线和测试线/1368.pdf","","多叠接双香蕉插头至多叠接香蕉插头","将电源或测试设备连接到面包板的理想选择","48in(1.2m)","多叠接双香蕉插头","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","NA","NA","300V","NA"]
["627","跳线和测试线","香蕉插头","/跳线和测试线/1368.jpg","1368-A-60","/跳线和测试线/1368.pdf","","多叠接双香蕉插头至多叠接香蕉插头","将电源或测试设备连接到面包板的理想选择","60in(1.5m)","多叠接双香蕉插头","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","NA","NA","300V","NA"]
["628","跳线和测试线","香蕉插头","/跳线和测试线/1326.jpg","1326-A-60","/跳线和测试线/1326-A.pdf","","多叠接双香蕉插头（仅一端）","1.此双香蕉插头电缆设计用于标准直径（4毫米）的香蕉插孔;\r\n2.可用于大多数数字万用表；\r\n3.该电缆也适用于具有接线柱输出的电源。","60in(1.5m)","多叠接双香蕉插头","NA","弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","双绞线","NA","NA","300VAC/424VDC","NA"]
["629","跳线和测试线","香蕉插头","/跳线和测试线/1326.jpg","1326-C-60","/跳线和测试线/1326-A.pdf","","多叠接双香蕉插头（仅一端）","1.此双香蕉插头电缆设计用于标准直径（4毫米）的香蕉插孔;\r\n2.可用于大多数数字万用表；\r\n3.该电缆也适用于具有接线柱输出的电源;4.香蕉头直径5.33mm。","60in(1.5m)","多叠接双香蕉插头","NA","弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","500V","NA"]
["630","跳线和测试线","香蕉插头","/跳线和测试线/5302.jpg","5302-12-*","/跳线和测试线/5302.pdf","","多叠接香蕉插头至SMD测试夹","1.非常适合用于表面安装设备的临时连接器以测试设备；\r\n2.香蕉插头可垂直堆叠和交叉堆叠。","12in(0.3m)","单香蕉插头","单SMD测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；抓钩：镀金不锈钢","最高+55℃(+131°F) \r\n ","22AWG","NA","5A","150V","NA"]
["631","跳线和测试线","香蕉插头","/跳线和测试线/5302.jpg","5302-24-*","/跳线和测试线/5302.pdf","","多叠接香蕉插头至SMD测试夹","1.非常适合用于表面安装设备的临时连接器以测试设备；\r\n2.香蕉插头可垂直堆叠和交叉堆叠。","24in(0.6m)","单香蕉插头","单SMD测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；抓钩：镀金不锈钢","最高+55℃(+131°F) \r\n ","22AWG","NA","5A","150V","NA"]
["632","跳线和测试线","香蕉插头","/跳线和测试线/5302.jpg","5302-36-*","/跳线和测试线/5302.pdf","","多叠接香蕉插头至SMD测试夹","1.非常适合用于表面安装设备的临时连接器以测试设备；\r\n2.香蕉插头可垂直堆叠和交叉堆叠。","36in(0.9m)","单香蕉插头","单SMD测试夹","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜；抓钩：镀金不锈钢","最高+55℃(+131°F) \r\n ","22AWG","NA","5A","150V","NA"]
["633","跳线和测试线","香蕉插头","/跳线和测试线/2239.jpg","2239-C-24","/跳线和测试线/2239.pdf","","多叠接香蕉插头（每端两个）","1.香蕉插头直径为5.33mm。","24in(0.6m)","多叠接单香蕉插头两个","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG/RG58C/U","NA","NA","1400V","NA"]
["634","跳线和测试线","香蕉插头","/跳线和测试线/2239.jpg","2239-C-36","/跳线和测试线/2239.pdf","","多叠接香蕉插头（每端两个）","1.香蕉插头直径为5.33mm。","36in(0.9m)","多叠接单香蕉插头两个","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG/RG58C/U","NA","NA","1400V","NA"]
["635","跳线和测试线","香蕉插头","/跳线和测试线/2239.jpg","2239-C-48","/跳线和测试线/2239.pdf","","多叠接香蕉插头（每端两个）","1.香蕉插头直径为5.33mm。","48in(1.2m)","多叠接单香蕉插头两个","多叠接单香蕉插头两个","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG/RG58C/U","NA","NA","1400V","NA"]
["636","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BA-18","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异；3.双绞线。","18in(0.5m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","NA","NA","300V","NA"]
["637","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BA-24","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异；3.双绞线。","24in(0.6m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","NA","NA","300V","NA"]
["638","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BA-36","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异；3.双绞线。","36in(0.9m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","NA","NA","300V","NA"]
["639","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BA-48","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异；3.双绞线。","48in(1.2m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","NA","NA","300V","NA"]
["640","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BA-60","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异；3.双绞线。","60in(1.5m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","18AWG","NA","NA","300V","NA"]
["641","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BC-24","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异。","24in(0.6m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","1400V","NA"]
["642","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BC-36","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异。","36in(0.9m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","1400V","NA"]
["643","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BC-48","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异。","48in(1.2m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","1400V","NA"]
["644","跳线和测试线","香蕉插头","/跳线和测试线/2BA.jpg","2BC-60","/跳线和测试线/2BA-2BC.pdf","","多叠接香蕉插头电缆","1.适合小信号测量；2.屏蔽性能优异。","60in(1.5m)","多叠接双香蕉插头","多叠接双香蕉插头","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","最高+55℃(+131°F) \r\n ","RG58C/U","NA","NA","1400V","NA"]
["645","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-6-*","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","6in(0.15m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-10℃至+55℃（+14℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["646","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-9-4","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","9in(0.23m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["647","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-12-*","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","12in(0.3m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["648","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-20-4","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","20in(0.5m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["649","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-24-*","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","24in(0.6m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["650","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-36-*","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","36in(0.9m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["651","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-72-*","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","72in(1.8m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["652","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-150-4","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","150in(3.8m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["653","跳线和测试线","香蕉插头","/跳线和测试线/73087.jpg","73087-210-4","/跳线和测试线/73087.pdf","","跳线测试线组","1.每套跳线测试导线包括一根带护套的4mm香蕉插头至带护套的4mm香蕉插头测试线，以及一根带护套的4mm香蕉插头至带护套的4mm香蕉插孔跳线；\r\n2.灵活的跳线测试引线组非常适合在最终连接之前通过测试点检查进行对等检查系统测试；\r\n3.插头和外壳采用一体式整体设计直接模制到电缆上，并且电线经过双重压接，可实现持久连接；4.低接触电阻；\r\n5.高股数硅胶绝缘电线具有出色的柔韧性和耐高温性。","210in(5.3m)","双香蕉插头","香蕉插头/插孔","香蕉插头：镀镍黄铜；弹簧：镀镍铍铜","-20℃至+55℃（-4℉至+131℉）","18AWG","NA","10A","CATⅠ1000V","NA"]
["654","跳线和测试线","香蕉插头","/跳线和测试线/2BC-PP.jpg","2BC-PP-36","/跳线和测试线/2BC-PP.pdf","","双香蕉插头至叠接管脚插头","1.将双香蕉插头快速转至两个管脚插头；2.管脚插头主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；3.线缆长度0.9m","36in(0.9m)","双香蕉插头","两个叠接管脚插头","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n管脚插头：主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","30VAC/60VDC","8A","1400V","NA"]
["655","跳线和测试线","香蕉插头","/跳线和测试线/2BC-PP.jpg","2BC-PP-48","/跳线和测试线/2BC-PP.pdf","","双香蕉插头至叠接管脚插头","1.将双香蕉插头快速转至两个管脚插头；2.管脚插头主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；3.线缆长度1.2m","48in(1.2m)","双香蕉插头","两个叠接管脚插头","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n管脚插头：主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","30VAC/60VDC","8A","1400V","NA"]
["656","跳线和测试线","香蕉插头","/跳线和测试线/2BC-PP.jpg","2BC-PP-60","/跳线和测试线/2BC-PP.pdf","","双香蕉插头至叠接管脚插头","1.将双香蕉插头快速转至两个管脚插头；2.管脚插头主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；3.线缆长度 1.5m","60in(1.5m)","双香蕉插头","两个叠接管脚插头","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n管脚插头：主体：镀金黄铜，弹簧：镀金铍铜，化学镀镍；","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","30VAC/60VDC","8A","1400V","NA"]
["657","跳线和测试线","鳄鱼夹","/跳线和测试线/3027-K.jpg","3027-K-24","/跳线和测试线/3027-K.pdf","","Minigator测试夹至小型双香蕉插头","1.鳄鱼夹开口：4.75mm","24in(0.6m)","小型双香蕉插头","鳄鱼夹","NA","最高+50℃(+122°F) \r\n ","RG174/U","30VAC/60VDC","8A","45V","NA"]
["658","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-8-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","8in(0.2m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["659","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-12-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","12in(0.3m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["660","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-18-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","18in(0.5m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["661","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-24-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","24in(0.6m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["662","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-36-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","36in(0.9m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["663","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-48-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","48in(1.2m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["664","跳线和测试线","测试夹","/跳线和测试线/3781.jpg","3781-60-*","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线","1.非常适合做临时跳线；\r\n2.提供极好的连接端子和绕线杆。","60in(1.5m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["665","跳线和测试线","小型香蕉插头","/跳线和测试线/2247-K.jpg","2247-K-24","/跳线和测试线/2247-K.pdf","","小型双香蕉插头电缆","1. 小型双香蕉接头的快速转接\r\n2. 镀金优选材质","24in(0.6m)","小型双香蕉插头","小型双香蕉插头","主体：镀金黄铜，弹簧:镀金铍铜","最高+55℃(+131°F) \r\n ","RG174/U","30VAC/60VDC","NA","1000V","NA"]
["666","跳线和测试线","测试夹","/跳线和测试线/5523.jpg","5523","/跳线和测试线/3781-5523.pdf","","Minigrabber测试夹跳线套件","1.包含20个 3781-24，10种颜色各一个\r\n2.非常适合提供临时跳线；\r\n3.提供极好的连接端子和绕线杆的连接器。","24in(0.6m)","单迷你测试夹","单迷你测试夹","主体：镀金铍铜，测试夹弹簧：不锈钢；\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0-9"]
["667","跳线和测试线","测试夹","/跳线和测试线/3780.jpg","3780-60-*","/跳线和测试线/3780.pdf","","Minigrabber®测试夹，仅一端","1.Minigrabber?测试夹(仅一端)允许定制开端；\r\n2.抓斗连接到1.060”(1.5 mm)的终端上；\r\n3.钩材为镀金铍铜，强度高，接触电阻低，保证信号完整性。\r\n4.为增加安全性，抓斗本体材料为阻燃尼龙6。\r\n5.不锈钢抓具压缩弹簧耐腐蚀，在整个抓具使用寿命中保持坚固感；\r\n6.多股线直接模压到抓爪执行机构帽和针头插头上，以保证耐用性。","60in(1.5m)","单迷你测试夹","NA","主体：镀金铍铜；弹簧：不锈钢；\r\n\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","8A","300V","0、2"]
["668","跳线和测试线","香蕉插头","/跳线和测试线/2BA-AL.jpg","2BA-AL-36","/跳线和测试线/2BA-AL_2BC-AL.pdf","","双香蕉插头至鳄鱼夹","1 将双香蕉插头快速转至两个鳄鱼夹","36in(0.9m)","双香蕉插头","两个鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧:镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","33VAC/70VDC","5A","150V","NA"]
["669","跳线和测试线","香蕉插头","/跳线和测试线/2BA-AL.jpg","2BA-AL-48","/跳线和测试线/2BA-AL_2BC-AL.pdf","","双香蕉插头至鳄鱼夹","1 将双香蕉插头快速转至两个鳄鱼夹","48in(1.2m)","双香蕉插头","两个鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧:镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG/引线：20AWG","33VAC/70VDC","5A","150V","NA"]
["670","跳线和测试线","香蕉插头","/跳线和测试线/2BA-AL.jpg","2BC-AL-36","/跳线和测试线/2BA-AL_2BC-AL.pdf","","双香蕉插头至鳄鱼夹","1 将双香蕉插头快速转至两个鳄鱼夹","36in(0.9m)","双香蕉插头","两个鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧:镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","33VAC/70VDC","5A","150V","NA"]
["671","跳线和测试线","香蕉插头","/跳线和测试线/2BA-AL.jpg","2BC-AL-60","/跳线和测试线/2BA-AL_2BC-AL.pdf","","双香蕉插头至鳄鱼夹","1 将双香蕉插头快速转至两个鳄鱼夹","60in(1.5m)","双香蕉插头","两个鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧:镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","RG58/引线：20AWG","33VAC/70VDC","5A","150V","NA"]
["672","跳线和测试线","低热电势跳线","/跳线和测试线/1756.jpg","1756-24","/跳线和测试线/1756.pdf","","屏蔽型低热电势（EMF）接线片跳线","1.理想的低压精密测量附件\r\n2.接线片为高导电性，镀金ETP铜110合金，可大大降低热电压(热EMF)的影响；\r\n3.热电动势在不同温度下不同金属接触时产生，是低微和纳伏测量中常见的误差来源；\r\n4.低热电势电动势接线片附在线屏蔽上以减少干扰、相互作用或泄漏等可能影响精确电压测量；\r\n5、带屏蔽线","24in(0.6m)","接线片","接线片","接线片：ETP(电解坚韧沥青)：镀金铜合金","最高+55℃(+131°F) \r\n ","12AWG/屏蔽线:18AWG","30VAC/60VDC","20A","2000V","NA"]
["673","跳线和测试线","低热电势跳线","/跳线和测试线/1756.jpg","1756-48","/跳线和测试线/1756.pdf","","屏蔽型低热电势（EMF）接线片跳线","1.理想的低压精密测量附件\r\n2.接线片为高导电性，镀金ETP铜110合金，可大大降低热电压(热EMF)的影响；\r\n3.热电动势在不同温度下不同金属接触时产生，是低微和纳伏测量中常见的误差来源；\r\n4.低热电势电动势接线片附在线屏蔽上以减少干扰、相互作用或泄漏等可能影响精确电压测量；\r\n5、带屏蔽线","48in(1.2m)","接线片","接线片","接线片：ETP(电解坚韧沥青)：镀金铜合金","最高+55℃(+131°F) \r\n ","12AWG/屏蔽线:18AWG","30VAC/60VDC","20A","2000V","NA"]
["674","跳线和测试线","低热电势跳线","/跳线和测试线/5295.jpg","5295-36-*","/跳线和测试线/5295.pdf","","低热电势（EMF）伸缩式护套香蕉插头至平接线片","1.适合低电压精密测量；\r\n2.设计可极大地减小热电压(热EMF)的影响；热电动势在不同温度、不同金属的触点产生，是低微和纳伏测量中常见的误差来源；\r\n3.香蕉插头材料采用镀金碲铜本体和镀金铍铜弹簧，用于低热电动势；\r\n4.接线片为高导电性电解坚韧沥青(ETP)， 110铜合金；\r\n5.香蕉插头采用可伸缩套设计，适用于安全护套或非护套插头。\r\n6.香蕉插头连接到低电阻多股（12）表线上。","36in(0.9m)","接线片","单香蕉插头","可伸缩护套香蕉插头：主体：镀金碲铜，弹簧：镀金铍铜；压缩弹簧：不锈钢；\r\n接线片：ETP(电解坚韧沥青)：镀金铜合金","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","7A"," 1000V","0、2"]
["675","跳线和测试线","低热电势跳线","/跳线和测试线/1693.jpg","1693-36-*","/跳线和测试线/1693.pdf","","低热电势（EMF)接线片跳线","1.适用于低压精密测量的测试附件；\r\n2.高导电性镀金ETP铜合金110接线片，连接到低电阻多股12规格线上；\r\n3.这种设计极大地减小了热电压(热EMF)的影响，热电动势产生于不同的金属在不同的温度时，是一个常见的误差来源在低微和纳伏的测量；","36in(0.9m)","接线片","接线片","接线片：ETP(电解坚韧沥青)：镀金铜合金","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","20A","2000V","0、2"]
["676","跳线和测试线","低热电势跳线","/跳线和测试线/1693.jpg","1693-60-*","/跳线和测试线/1693.pdf","","低热电势（EMF)接线片跳线","1.适用于低压精密测量的测试附件；\r\n2.高导电性镀金ETP铜合金110接线片，连接到低电阻多股12规格线上；\r\n3.这种设计极大地减小了热电压(热EMF)的影响，热电动势产生于不同的金属在不同的温度时，是一个常见的误差来源在低微和纳伏的测量；","60in(1.5m)","接线片","接线片","接线片：ETP(电解坚韧沥青)：镀金铜合金","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","20A","2000V","0、2"]
["677","跳线和测试线","低热电势跳线","/跳线和测试线/5291A.jpg","5291A-24-*","/跳线和测试线/5291A.pdf","","低热电势（EMF)伸缩式护套香蕉插头跳线","1.适用于低压精密测量的测试附件；\r\n2 极大地减小了热电压(热EMF)的影响\r\n3 香蕉插头带绝缘头","12in(0.3m)","单香蕉插头","单香蕉插头","伸缩护套香蕉插头:主体：镀金碲铜，弹簧：镀金铍铜；压缩弹簧：不锈钢","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","7A","1000V","0、2"]
["678","跳线和测试线","低热电势跳线","/跳线和测试线/5291A.jpg","5291A-36-*","/跳线和测试线/5291A.pdf","","低热电势（EMF)伸缩式护套香蕉插头跳线","1.适用于低压精密测量的测试附件；\r\n2 极大地减小了热电压(热EMF)的影响\r\n3 香蕉插头带绝缘头","36in(0.9m)","单香蕉插头","单香蕉插头","伸缩护套香蕉插头:主体：镀金碲铜，弹簧：镀金铍铜；压缩弹簧：不锈钢","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","7A","1000V","0、2"]
["679","跳线和测试线","低热电势跳线","/跳线和测试线/5291A.jpg","5291A-60-*","/跳线和测试线/5291A.pdf","","低热电势（EMF)伸缩式护套香蕉插头跳线","1.适用于低压精密测量的测试附件；\r\n2 极大地减小了热电压(热EMF)的影响\r\n3 香蕉插头带绝缘头","60in(1.5m)","单香蕉插头","单香蕉插头","伸缩护套香蕉插头弹簧：镀铍铜；压缩弹簧：不锈钢\r\n绝缘：聚丙烯","最高+55℃(+131°F) \r\n ","12AWG\r\n","30VAC/60VDC","7A","1000V","0、2"]
["680","跳线和测试线","测试夹","/跳线和测试线/5301.jpg","5301-12-*","/跳线和测试线/5301-5521.pdf","","SMD Grabber测试夹跳线","1 适合表面安装的器件测试\r\n","12in(0.3m)","单测试夹","单测试夹","镀金不锈钢\r\n","最高+102℃(+216°F)","12AWG\r\n"," 33VAC/70VDC","0.5A","150V","0、2"]
["681","跳线和测试线","测试夹","/跳线和测试线/5301.jpg","5301-24-*","/跳线和测试线/5301-5521.pdf","","SMD Grabber测试夹跳线","1 适合表面安装的器件测试\r\n","24in(0.6m)","单测试夹","单测试夹","镀金不锈钢\r\n","最高+102℃(+216°F)","12AWG\r\n"," 33VAC/70VDC","0.5A","150V","0、2"]
["682","跳线和测试线","测试夹","/跳线和测试线/5521.jpg","5521","/跳线和测试线/5301-5521.pdf","","SMD Grabber 测试夹跳线套件","1 适合表面安装的器件测试\r\n2 SMD测试夹跳线组件，10种颜色各一个","24in(0.6m)","单测试夹","单测试夹","镀金不锈钢\r\n","最高+102℃(+216°F)","12AWG\r\n"," 33VAC/70VDC","0.5A","150V","0-9"]
["683","跳线和测试线","鳄鱼夹","/跳线和测试线/6576.jpg","6576-24-*","/跳线和测试线/5301-5521.pdf","","1000V鳄鱼夹跳线","1.在电路之间建立临时连接的理想选择；\r\n2.多种电线长度；\r\n3.鳄鱼夹可固定在外径最大为0.300英寸（7.62毫米）的物体上。\r\n4.耐热的Santoprene橡胶和硅树脂制成。","24in(0.6m)","单鳄鱼夹","单鳄鱼夹","主体：镀镍钢，护套：Santoprene橡胶\r\n","-25℃至+80℃（-13℉至+176℉）","18AWG","30VAC/60VDC","10A","1000V","0、2"]
["684","跳线和测试线","鳄鱼夹","/跳线和测试线/6576.jpg","6576-36-*","/跳线和测试线/5301-5521.pdf","","1000V鳄鱼夹跳线","1.在电路之间建立临时连接的理想选择；\r\n2.多种电线长度；\r\n3.鳄鱼夹可固定在外径最大为0.300英寸（7.62毫米）的物体上。\r\n4.耐热的Santoprene橡胶和硅树脂制成。","36in(0.9m)","单鳄鱼夹","单鳄鱼夹","主体：镀镍钢，护套：Santoprene橡胶\r\n","-25℃至+80℃（-13℉至+176℉）","18AWG","30VAC/60VDC","10A","1000V","0、2"]
["685","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","1166-12-*","/跳线和测试线/1166-6357.pdf","","多叠接单香蕉插头至鳄鱼夹","1.可堆叠香蕉插头跳线的鳄鱼夹可快速连接至外径为0.3英寸（7.62毫米）的端子；\r\n2.跳线具有中等大小的鳄鱼夹和可弯曲的护套，可提供绝缘保护;3.香蕉插头弹簧是铍铜，可延长插入寿命;\r\n4.香蕉插头具有垂直和水平堆叠功能;\r\n5.导线具有多股绞线，具有出色的导线柔韧性;\r\n6.香蕉插头直接模制到电线上以增加拉力。","12in(0.3m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]
["686","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","1166-24-*","/跳线和测试线/1166-6357.pdf","","多叠接单香蕉插头至鳄鱼夹","1.可堆叠香蕉插头跳线的鳄鱼夹可快速连接至外径为0.3英寸（7.62毫米）的端子；\r\n2.跳线具有中等大小的鳄鱼夹和可弯曲的护套，可提供绝缘保护;3.香蕉插头弹簧是铍铜，可延长插入寿命;\r\n4.香蕉插头具有垂直和水平堆叠功能;\r\n5.导线具有多股绞线，具有出色的导线柔韧性;\r\n6.香蕉插头直接模制到电线上以增加拉力。","24in(0.6m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]
["687","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","1166-36-*","/跳线和测试线/1166-6357.pdf","","多叠接单香蕉插头至鳄鱼夹","1.可堆叠香蕉插头跳线的鳄鱼夹可快速连接至外径为0.3英寸（7.62毫米）的端子；\r\n2.跳线具有中等大小的鳄鱼夹和可弯曲的护套，可提供绝缘保护;3.香蕉插头弹簧是铍铜，可延长插入寿命;\r\n4.香蕉插头具有垂直和水平堆叠功能;\r\n5.导线具有多股绞线，具有出色的导线柔韧性;\r\n6.香蕉插头直接模制到电线上以增加拉力。","36in(0.9m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]
["688","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","1166-48-*","/跳线和测试线/1166-6357.pdf","","多叠接单香蕉插头至鳄鱼夹","1.可堆叠香蕉插头跳线的鳄鱼夹可快速连接至外径为0.3英寸（7.62毫米）的端子；\r\n2.跳线具有中等大小的鳄鱼夹和可弯曲的护套，可提供绝缘保护;3.香蕉插头弹簧是铍铜，可延长插入寿命;\r\n4.香蕉插头具有垂直和水平堆叠功能;\r\n5.导线具有多股绞线，具有出色的导线柔韧性;\r\n6.香蕉插头直接模制到电线上以增加拉力。","48in(1.2m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]
["689","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","1166-60-*","/跳线和测试线/1166-6357.pdf","","多叠接单香蕉插头至鳄鱼夹","1.可堆叠香蕉插头跳线的鳄鱼夹可快速连接至外径为0.3英寸（7.62毫米）的端子；\r\n2.跳线具有中等大小的鳄鱼夹和可弯曲的护套，可提供绝缘保护;3.香蕉插头弹簧是铍铜，可延长插入寿命;\r\n4.香蕉插头具有垂直和水平堆叠功能;\r\n5.导线具有多股绞线，具有出色的导线柔韧性;\r\n6.香蕉插头直接模制到电线上以增加拉力。","60in(1.5m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]
["690","跳线和测试线","香蕉插头","/跳线和测试线/1166.jpg","6357-36","/跳线和测试线/1166-6357.pdf","","多香蕉单插头至鳄鱼夹跳线套件","1166-36型跳线10种颜色各一个","36in(0.9m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0-9"]
["691","跳线和测试线","测试夹","/跳线和测试线/4613.jpg","4613-12-*","/跳线和测试线/4613-5525.pdf","","MicroGrabber微型测试夹跳线","在小型组件之间提供跨接线的理想选择；","12in(0.3m)","单测试夹","单测试夹","主体：镀金铍铜，弹簧：镀金不锈钢\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","3A","150V","0、2"]
["692","跳线和测试线","测试夹","/跳线和测试线/4613.jpg","4613-24-*","/跳线和测试线/4613-5525.pdf","","MicroGrabber微型测试夹跳线","在小型组件之间提供跨接线的理想选择；","24in(0.6m)","单测试夹","单测试夹","主体：镀金铍铜，弹簧：镀金不锈钢\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","3A","150V","0、2"]
["693","跳线和测试线","测试夹","/跳线和测试线/4613.jpg","4613-36-*","/跳线和测试线/4613-5525.pdf","","MicroGrabber微型测试夹跳线","在小型组件之间提供跨接线的理想选择；","36in(0.9m)","单测试夹","单测试夹","主体：镀金铍铜，弹簧：镀金不锈钢\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","3A","150V","0、2"]
["694","跳线和测试线","测试夹","/跳线和测试线/4613.jpg","4613-48-*","/跳线和测试线/4613-5525.pdf","","MicroGrabber微型测试夹跳线","在小型组件之间提供跨接线的理想选择；","48in(1.2m)","单测试夹","单测试夹","主体：镀金铍铜，弹簧：镀金不锈钢\r\n","最高+102℃(+216°F)","20AWG","30VAC/60VDC","3A","150V","0、2"]
["695","跳线和测试线","测试夹","/跳线和测试线/5525.jpg","5525","/跳线和测试线/4613-5525.pdf","","MicroGrabber微型测试夹跳线套件","套件包含10件4613-24型，每种颜色各一个。","24in(0.6m)","单测试夹","单测试夹","主体：镀金铍铜，弹簧：镀金不锈钢\r\n","","20AWG","30VAC/60VDC","3A","150V","0-9"]
["696","跳线和测试线","鳄鱼夹","/跳线和测试线/MG-B.jpg","MG-B-12-*","/跳线和测试线/MG-B.pdf","","Minigator型测试夹跳线","1.具有用于绝缘保护的软靴；\r\n2.鳄鱼夹镀镍以防变色；\r\n3.鳄鱼夹最大开口为.187英寸（4.75毫米）;\r\n4.理想用作临时电线。","12in(0.3m)","单鳄鱼夹","单鳄鱼夹","主体：镀镍钢 弹簧：不锈钢\r\n","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A","45V","0、2"]
["697","跳线和测试线","鳄鱼夹","/跳线和测试线/MG-B.jpg","MG-B-24-*","/跳线和测试线/MG-B.pdf","","Minigator型测试夹跳线","1.具有用于绝缘保护的软靴；\r\n2.鳄鱼夹镀镍以防变色；\r\n3.鳄鱼夹最大开口为.187英寸（4.75毫米）;\r\n4.理想用作临时电线。","24in(0.6m)","单鳄鱼夹","单鳄鱼夹","主体：镀镍钢 弹簧：不锈钢\r\n","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A","45V","0、2"]
["698","跳线和测试线","鳄鱼夹","/跳线和测试线/AL-B.jpg","AL-B-12-*","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线","1.非常适合用作临时跳线;\r\n2.鳄鱼夹钳口可打开至7.62mm。","12in(0.3m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0、2"]
["699","跳线和测试线","鳄鱼夹","/跳线和测试线/AL-B.jpg","AL-B-24-*","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线","1.非常适合用作临时跳线;\r\n2.鳄鱼皮钳口可打开至7.62mm。","24in(0.6m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0、2"]
["700","跳线和测试线","鳄鱼夹","/跳线和测试线/AL-B.jpg","AL-B-36-*","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线","1.非常适合用作临时跳线;\r\n2.鳄鱼皮钳口可打开至7.62mm。","36in(0.9m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0、2"]
["701","跳线和测试线","鳄鱼夹","/跳线和测试线/AL-B.jpg","AL-B-48-*","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线","1.非常适合用作临时跳线;\r\n2.鳄鱼皮钳口可打开至7.62mm。","48in(1.2m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0、2"]
["702","跳线和测试线","鳄鱼夹","/跳线和测试线/AL-B.jpg","AL-B-60-*","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线","1.非常适合用作临时跳线;\r\n2.鳄鱼皮钳口可打开至7.62mm。","60in(1.5m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0、2"]
["703","跳线和测试线","鳄鱼夹","/跳线和测试线/6356.jpg","6356-12","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线套件","1.非常适合用作临时跳线;\r\n2.鳄鱼夹钳口可打开至7.62mm。\r\n3. AL-B-12 型号10种颜色各1个的组合套件","12in(0.3m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0-9"]
["704","跳线和测试线","鳄鱼夹","/跳线和测试线/6356.jpg","6356-24","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线套件","1.非常适合用作临时跳线;\r\n2.鳄鱼夹钳口可打开至7.62mm。\r\n3. AL-B-24 型号10种颜色各1个的组合套件","24in(0.6m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0-9"]
["705","跳线和测试线","鳄鱼夹","/跳线和测试线/6356.jpg","6356-36","/跳线和测试线/AL-B-6356.pdf","","鳄鱼夹跳线套件","1.非常适合用作临时跳线;\r\n2.鳄鱼夹钳口可打开至7.62mm。\r\n3. AL-B-36 型号10种颜色各1个的组合套件","36in(0.9m)","单鳄鱼夹","单鳄鱼夹","镀镍钢","最高+50℃(+122°F) \r\n ","18AWG","33VAC/70VDC","5A"," 150V","0-9"]
["706","跳线和测试线","鳄鱼夹","/跳线和测试线/6483-48-02.jpg","6483-48-02","/跳线和测试线/6483-48-02.pdf","","5向鳄鱼夹至带护套的直角香蕉插头套件","1.多功能测试夹允许通过五种方式连接到被测设备；\r\n2.U型鼻，用于叶片形端子；\r\n3.带槽的钳口，用于夹紧螺丝头，裸线或端子；\r\n4.锯齿状的齿，用于夹持螺纹或绕线端子；\r\n5.锐利的针束，用于刺穿小规格导线（22-28 AWG）；\r\n6.大型穿刺针，可穿透大规格导线。","48in(1.2m)","单鳄鱼夹","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：：抗锈镍铜合金","NA","18AWG","30VAC/60VDC","8A","300V","0、2"]
["707","跳线和测试线","香蕉插头","/跳线和测试线/3220.jpg","3220-12-*","/跳线和测试线/3220.pdf","","多叠接香蕉插头至Minigator测试夹","1.提供用于交叉堆叠的横孔，以及用于垂直堆叠的插孔；\r\n2.允许从香蕉插孔使用带引线的鳄鱼夹。","12in(0.3m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：：镀镍钢","最高+50℃(+122°F) \r\n ","20AWG","30VAC/60VDC","5A","45V","0、2"]
["708","跳线和测试线","香蕉插头","/跳线和测试线/3220.jpg","3220-24-*","/跳线和测试线/3220.pdf","","多叠接香蕉插头至Minigator测试夹","1.提供用于交叉堆叠的横孔，以及用于垂直堆叠的插孔；\r\n2.允许从香蕉插孔使用带引线的鳄鱼夹。","24in(0.6m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：：镀镍钢","最高+50℃(+122°F) \r\n ","20AWG","30VAC/60VDC","5A","45V","0、2"]
["709","跳线和测试线","香蕉插头","/跳线和测试线/3220.jpg","3220-36-*","/跳线和测试线/3220.pdf","","多叠接香蕉插头至Minigator测试夹","1.提供用于交叉堆叠的横孔，以及用于垂直堆叠的插孔；\r\n2.允许从香蕉插孔使用带引线的鳄鱼夹。","36in(0.9m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：：镀镍钢","最高+50℃(+122°F) \r\n ","20AWG","30VAC/60VDC","5A","45V","0、2"]
["710","跳线和测试线","香蕉插头","/跳线和测试线/3220.jpg","3220-48-*","/跳线和测试线/3220.pdf","","多叠接香蕉插头至Minigator测试夹","1.提供用于交叉堆叠的横孔，以及用于垂直堆叠的插孔；\r\n2.允许从香蕉插孔使用带引线的鳄鱼夹。","48in(1.2m)","单多叠接香蕉插头","单鳄鱼夹","香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；\r\n鳄鱼夹：：镀镍钢","最高+50℃(+122°F) \r\n ","20AWG","30VAC/60VDC","5A","45V","0、2"]
["711","跳线和测试线","香蕉插头","/跳线和测试线/4911A.jpg","4911A-12-*","/跳线和测试线/4911A.pdf","","伸缩式护套香蕉插头跳线","1.可伸缩的护套端允许与标准护套或非护套型香蕉1.66英寸（4毫米）插孔接口；\r\n2.插头和外壳以一体式整体设计直接模制到电缆上，导线双重压接，可实现持久连接；\r\n3.多叶香蕉弹簧材料是铍铜，镀镍以延长插入寿命并降低接触电阻；\r\n4.测试线可以与各种各样的Pomona探针，鳄鱼夹，平接片等配合。","12in(0.3m)","单香蕉插头","单香蕉插头","伸缩护套香蕉弹簧：主体：镀镍黄铜，弹片：镀镍铍铜；压缩弹簧：不锈钢；","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","10A","CATⅢ 1000V","0、2"]
["712","跳线和测试线","香蕉插头","/跳线和测试线/4911A.jpg","4911A-24-*","/跳线和测试线/4911A.pdf","","伸缩式护套香蕉插头跳线","1.可伸缩的护套端允许与标准护套或非护套型香蕉1.66英寸（4毫米）插孔接口；\r\n2.插头和外壳以一体式整体设计直接模制到电缆上，导线双重压接，可实现持久连接；\r\n3.多叶香蕉弹簧材料是铍铜，镀镍以延长插入寿命并降低接触电阻；\r\n4.测试线可以与各种各样的Pomona探针，鳄鱼夹，平接片等配合。","24in(0.6m)","单香蕉插头","单香蕉插头","伸缩护套香蕉弹簧：主体：镀镍黄铜，弹片：镀镍铍铜；压缩弹簧：不锈钢；","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","10A","CATⅢ 1000V","0、2"]
["713","跳线和测试线","香蕉插头","/跳线和测试线/4911A.jpg","4911A-36-*","/跳线和测试线/4911A.pdf","","伸缩式护套香蕉插头跳线","1.可伸缩的护套端允许与标准护套或非护套型香蕉1.66英寸（4毫米）插孔接口；\r\n2.插头和外壳以一体式整体设计直接模制到电缆上，导线双重压接，可实现持久连接；\r\n3.多叶香蕉弹簧材料是铍铜，镀镍以延长插入寿命并降低接触电阻；\r\n4.测试线可以与各种各样的Pomona探针，鳄鱼夹，平接片等配合。","36in(0.9m)","单香蕉插头","单香蕉插头","伸缩护套香蕉弹簧：主体：镀镍黄铜，弹片：镀镍铍铜；压缩弹簧：不锈钢；","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","10A","CATⅢ 1000V","0、2"]
["714","跳线和测试线","香蕉插头","/跳线和测试线/4911A.jpg","4911A-48-*","/跳线和测试线/4911A.pdf","","伸缩式护套香蕉插头跳线","1.可伸缩的护套端允许与标准护套或非护套型香蕉1.66英寸（4毫米）插孔接口；\r\n2.插头和外壳以一体式整体设计直接模制到电缆上，导线双重压接，可实现持久连接；\r\n3.多叶香蕉弹簧材料是铍铜，镀镍以延长插入寿命并降低接触电阻；\r\n4.测试线可以与各种各样的Pomona探针，鳄鱼夹，平接片等配合。","48in(1.2m)","单香蕉插头","单香蕉插头","伸缩护套香蕉弹簧：主体：镀镍黄铜，弹片：镀镍铍铜；压缩弹簧：不锈钢；","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","10A","CATⅢ 1000V","0、2"]
["715","跳线和测试线","香蕉插头","/跳线和测试线/4911A.jpg","4911A-60-*","/跳线和测试线/4911A.pdf","","伸缩式护套香蕉插头跳线","1.可伸缩的护套端允许与标准护套或非护套型香蕉1.66英寸（4毫米）插孔接口；\r\n2.插头和外壳以一体式整体设计直接模制到电缆上，导线双重压接，可实现持久连接；\r\n3.多叶香蕉弹簧材料是铍铜，镀镍以延长插入寿命并降低接触电阻；\r\n4.测试线可以与各种各样的Pomona探针，鳄鱼夹，平接片等配合。","60in(1.5m)","单香蕉插头","单香蕉插头","伸缩护套香蕉弹簧：主体：镀镍黄铜，弹片：镀镍铍铜；压缩弹簧：不锈钢；","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","10A","CATⅢ 1000V","0、2"]
["716","跳线和测试线","测试夹","/跳线和测试线/4650.jpg","4650-24-*","/跳线和测试线/4650.pdf","","Minigraber测试夹至直插香蕉插头跳线","将端子和绕线柱连接到测试设备的理想选择。","24in(0.6m)","单测试夹","单香蕉插头","测试夹: 主体：镀金铍铜，弹簧：不锈钢；\r\n香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2"]
["717","跳线和测试线","测试夹","/跳线和测试线/4650.jpg","4650-36-*","/跳线和测试线/4650.pdf","","Minigraber测试夹至直插香蕉插头跳线","将端子和绕线柱连接到测试设备的理想选择。","36in(0.9m)","单测试夹","单香蕉插头","测试夹: 主体：镀金铍铜，弹簧：不锈钢；\r\n香蕉插头：主体：镀镍黄铜，弹簧：镀镍铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A","300V","0、2"]
["718","跳线和测试线","管脚插头/插孔","/跳线和测试线/4771.jpg","4771-24-*","/跳线和测试线/4771.pdf","","0.64mm方管脚插孔至直插香蕉插头","非常适合作为0.6 (0.025) sq 电路板管脚及直径4.2(.166)的引脚跳线。","24in(0.6m)","单方管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","30VAC/60VDC","3A","1000V","0、2"]
["719","跳线和测试线","管脚插头/插孔","/跳线和测试线/4771.jpg","4771-36-*","/跳线和测试线/4771.pdf","","0.64mm方管脚插孔至直插香蕉插头","非常适合作为0.6 (0.025) sq 电路板管脚及直径4.2(.166)的引脚跳线。","36in(0.9m)","单方管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","30VAC/60VDC","3A","1000V","0、2"]
["720","跳线和测试线","管脚插头/插孔","/跳线和测试线/4741.jpg","4741-6-*","/跳线和测试线/4741-5948.pdf","","0.64mm方管脚插孔至直插香蕉插头","1 接口适配Pomona .025”(.64mm) 方管脚微型测试夹(型号4521)，旋转型微型测试夹(型号5790)，SMD Grabber(型号5360)和Minigator(型号5363)。\r\n2 是 .025 \"(.64mm)的方管脚的理想跳线选择\r\n3 插孔是镀金的，以优化电气连接。","6in(0.15m)","单管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","45VAC/60VDC","3A","45V","0、2"]
["721","跳线和测试线","管脚插头/插孔","/跳线和测试线/4741.jpg","4741-12-*","/跳线和测试线/4741-5948.pdf","","0.64mm方管脚插孔至直插香蕉插头","1 接口适配Pomona .025”(.64mm) 方管脚微型测试夹(型号4521)，旋转型微型测试夹(型号5790)，SMD Grabber(型号5360)和Minigator(型号5363)。\r\n2 是 .025 \"(.64mm)的方管脚的理想跳线选择\r\n3 插孔是镀金的，以优化电气连接。","12in(0.3m)","单管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","45VAC/60VDC","3A","45V","0、2"]
["722","跳线和测试线","管脚插头/插孔","/跳线和测试线/4741.jpg","4741-24-*","/跳线和测试线/4741-5948.pdf","","0.64mm方管脚插孔至直插香蕉插头","1 接口适配Pomona .025”(.64mm) 方管脚微型测试夹(型号4521)，旋转型微型测试夹(型号5790)，SMD Grabber(型号5360)和Minigator(型号5363)。\r\n2 是 .025 \"(.64mm)的方管脚的理想跳线选择\r\n3 插孔是镀金的，以优化电气连接。","24in(0.6m)","单管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","45VAC/60VDC","3A","45V","0、2"]
["723","跳线和测试线","管脚插头/插孔","/跳线和测试线/4741.jpg","5948","/跳线和测试线/4741-5948.pdf","","0.64mm方管脚插孔至直插香蕉插头跳线套件","4741-6型，10种颜色各1套件","6in(0.15m)","单管脚插孔","单香蕉插头","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n管脚插孔：镀金磷青铜\r\n\r\n","最高+50℃(+122°F) \r\n ","22AWG","45VAC/60VDC","3A","45V","0-9"]
["724","跳线和测试线","香蕉插头","/跳线和测试线/4702.jpg","4702-24-*","/跳线和测试线/4702.pdf","","香蕉插头至香蕉插孔","1.当用作延长线时，绝缘所有热引线；\r\n2.连接器香蕉插头可补线延伸到连接器。","24in(0.6m)","单香蕉插头","单香蕉插孔","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n香蕉插孔：镀镍黄铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["725","跳线和测试线","香蕉插头","/跳线和测试线/4702.jpg","4702-36-*","/跳线和测试线/4702.pdf","","香蕉插头至香蕉插孔","1.当用作延长线时，绝缘所有热引线；\r\n2.连接器香蕉插头可补线延伸到连接器。","36in(0.9m)","单香蕉插头","单香蕉插孔","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n香蕉插孔：镀镍黄铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["726","跳线和测试线","香蕉插头","/跳线和测试线/4702.jpg","4702-48-*","/跳线和测试线/4702.pdf","","香蕉插头至香蕉插孔","1.当用作延长线时，绝缘所有热引线；\r\n2.连接器香蕉插头可补线延伸到连接器。","48in(1.2m)","单香蕉插头","单香蕉插孔","香蕉插头：主体：镀镍黄铜，弹片：镀镍铍铜；\r\n香蕉插孔：镀镍黄铜","最高+55℃(+131°F) \r\n ","18AWG","30VAC/60VDC","15A","5000V","0、2"]
["727","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-4-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","4in(0.1m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["728","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-8-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","8in(0.2m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["729","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-12-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","12in(0.3m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["730","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-18-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","18in(0.5m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["731","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-24-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","24in(0.6m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["732","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-36-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","36in(0.9m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["733","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-48-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","48in(1.2m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["734","跳线和测试线","小型香蕉插头","/跳线和测试线/1081.jpg","1081-60-*","/跳线和测试线/1081.pdf","","小型叠接香蕉插头跳线","1.香蕉插头弹簧材料为镀金铍铜，接触电阻低，插入寿命长；\r\n2.为了测试通用性，香蕉插头采用立式堆叠设计；\r\n3.钢丝绞线数采用多股，具有极佳的钢丝柔韧性；\r\n4.香蕉插头直接模压在电线上，增加拉力。","60in(1.5m)","单小型叠接香蕉插头","单小型叠接香蕉插头","主体：镀金黄铜，弹簧：镀金铍铜；","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["735","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-4-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","4in(0.1m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["736","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-8-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","8in(0.2m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["737","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-12-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","12in(0.3m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["738","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-18-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","18in(0.5m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["739","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-24-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","24in(0.6m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["740","跳线和测试线","管脚插头/插孔","/跳线和测试线/P.jpg","P-36-*","/跳线和测试线/P.pdf","","叠接管脚插头跳线","1 可堆叠管脚插头\r\n2 适配型号3542,4773或任何其他标准的.08英寸管脚插孔\r\n3 非常适合作为底盘盒上的跳线。","36in(0.9m)","单管脚插头","单管脚插头","镀金黄铜","最高+55℃(+131°F) \r\n ","20AWG","30VAC/60VDC","5A"," 3000V","0、2"]
["741","跳线和测试线","鳄鱼夹","/跳线和测试线/1960.jpg","1960-36-*","/跳线和测试线/1960.pdf","","鳄鱼夹至绝缘平接线片","1.平接线片安全地连接到一个螺钉终端，而中等大小的鳄鱼测试夹可以迅速抓住终端；\r\n2.平接线片和鳄鱼身体是镀镍的抗变色；\r\n3.鳄鱼夹有软性的靴子做绝缘保护；\r\n4.鳄鱼夹最大开口4.75毫米。","36in(0.9m)","单鳄鱼夹","单接线片","鳄鱼夹：主体：镀镍钢，弹簧:不锈钢；\r\n平接线片：镀镍黄铜","最高+50℃(+122°F) \r\n ","18AWG","30VAC/60VDC","5A","150V","0、2"]