{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Sheet0"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Sheet0","index":0,"n_rows":15,"n_cols":17,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["ID","一级","二级","图片路径","型号","PDF","URl","中文名称","特性","端A","端B","材质","标称阻抗","接触电阻","工作温度","手持测试最大电压","离手使用最大电压"]
["888","音频、视频、广播","BNC型","/音频、视频、广播/5319.jpg","5319","/音频、视频、广播/5319.pdf","","BNC母头至耳机（RCA）插头","1.允许标准BNC电缆(公端)与有唱机插孔的设备一起使用；\r\n2.镀金中心接点，最小的接触电阻和优越的信号传输；3.机加工(非压铸)部件，使用寿命长。","BNC母头","耳机（RCA）插头","阀体和外部触点:镀镍黄铜；\r\n中心接点-音频插头:镀金黄铜；\r\n中心接点- BNC母头:镀金铍铜","NA","NA","最高+102℃(+216℉)","33VAC/70VDC","500V"]
["889","音频、视频、广播","BNC型","/音频、视频、广播/4054.jpg","4054","/音频、视频、广播/4054.pdf","","BNC公头至耳机插孔","1.允许音频设备插头与一端为BNC母头的设备连接；\r\n2.采用金属结构，确保必要的屏蔽性能。","BNC公头","耳机插孔","插孔：镀镍黄铜；\r\nBNC 公头：镀镍黄铜；\r\n表面处理:阀体和配件，抗变色。\r\n中心触点:镀金","50Ω","NA","最高+125ºC(+257ºF)","NA","500V"]
["890","音频、视频、广播","BNC型","/音频、视频、广播/1297.jpg","1297","/音频、视频、广播/1297.pdf","","BNC母头至6.35mm耳机插头","1.实现电话设备与BNC的测试仪器之间的互连；\r\n2.可以方便地将BNC电缆匹配到设备的标准插孔；\r\n3.BNC(母)触点为镀金铍铜，无噪声连接；\r\n4.适配器具有良好的抗变色能力。","BNC母头","耳机插头","BNC(母头):阀体-黄铜，抗锈蚀\r\n中心联系人:镀金铍铜；插头(两导体):镀镍黄铜\r\n介质:聚四氟乙烯\r\n手柄:镀镍黄铜\r\n","50Ω","NA","最高 +125°C (+257°F)","NA","500V"]
["891","音频、视频、广播","BNC型","/音频、视频、广播/3837.jpg","3837","/音频、视频、广播/3837.pdf","","BNC母头至3.5mm迷你耳机插头","1.方便BNC公头与小插头的设备连接；\r\n2.适应现有BNC同轴电缆；\r\n3.采用金属结构，确保适当的屏蔽。","BNC母头","迷你耳机插头","BNC母头：阀体和配件:抗锈蚀；\r\n中心触点:镀金；\r\n主体：镀镍黄铜","NA","NA","‘-55℃至125℃(-67℉至+257℉)","NA","500V"]
["892","音频、视频、广播","PCB安装耳机插孔","/音频、视频、广播/7158.jpg","7158","/音频、视频、广播/7158.pdf","","6.35mmPCB安装耳机插孔","1.连接标准商业电话插头；\r\n2.可PC板安装；\r\n3.适用立体声和单声道；\r\n4.可焊接；\r\n5.带3个接触连接片；6.绝缘电阻1000MΩ，介电强度1000VDC","6.35mmPCB安装耳机插孔","NA","外壳:尼龙；\r\n接触片:镀镍银","NA","小于15mΩ","NA","NA","NA"]
["893","音频、视频、广播","PCB安装耳机插孔","/音频、视频、广播/7159.jpg","7159","/音频、视频、广播/7159.pdf","","6.35mmPCB安装耳机插孔","1.连接标准商业电话插头；\r\n2.可PC板安装；\r\n3.适用立体声和单声道；\r\n4.可焊接；\r\n5.带2个接触连接片；6.绝缘电阻1000MΩ，介电强度1000VDC","6.35mmPCB安装耳机插孔","NA","外壳:尼龙；\r\n接触片:镀镍银","NA","小于15mΩ","NA","NA","NA"]
["894","音频、视频、广播","PCB安装耳机插孔","/音频、视频、广播/7160.jpg","7160","/音频、视频、广播/7160.pdf","","6.35mmPCB安装耳机插孔","1.连接标准商业电话插头；\r\n2.可PC板安装；\r\n3.适用立体声和单声道；\r\n4.可焊接；\r\n5.带3个接触连接片；6.接触片有接线孔；7.绝缘电阻1000MΩ，介电强度1000VDC","6.35mmPCB安装耳机插孔","NA","外壳:尼龙；\r\n接触片:锡","NA","小于15mΩ","NA","NA","NA"]
["895","音频、视频、广播","BNC型","/音频、视频、广播/4043.jpg","4043","/音频、视频、广播/4043.pdf","","BNC公头至6.35mm(0.25in)两导体耳机插孔","1.标准2导体6.4mm(0.25in)电话插头与BNC母头的设备连接；\r\n2.采用金属结构，确保适当的屏蔽；3.插孔:两导体，屏蔽。","BNC公头","6.35mm耳机插孔","BNC公头阀体和配件：表面处理:抗变色；\r\n中心导体:镀金；主体:镀镍黄铜；\r\n插孔:镀镍黄铜","NA","NA","最高 +125°C (+257°F)","NA","NA"]
["896","音频、视频、广播","F型","/射频同轴连接器/6713.jpg","6713","/射频同轴连接器/6713.pdf","","F型公头至F型母头串联适配器","1.串联推入式，可快速可靠与F型母头连接器匹配；2.测试和制造的理想选择；3.接触电阻：最大3毫欧，绝缘电阻：最小5000MΩ；4.频率范围：0至500MHz；5.电压驻波比：≤1.5","F型公头","F型母头","主体：镀镍黄铜；中心触点：镀镍黄铜","NA","NA","‘-40℃至+65℃ （-40˚F至+149˚F）","33VAC/70VDC","500V"]
["897","音频、视频、广播","双香蕉插头","/音频、视频、广播/1442.jpg","1442","/音频、视频、广播/1442.pdf","","耳机插孔至叠接双香蕉插头","将设备BNC公头与有标准香蕉插头或接线柱的设备连接","BNC母头","双香蕉插头","\r\n绝缘材料:用聚丙烯\r\n双香蕉插头：弹簧：镀镍铍铜；阀体：镀镍黄铜；\r\n","NA","NA","最高+ 50℃(+ 122℉)","NA","500V"]
["898","音频、视频、广播","插头/插孔","/音频、视频、广播/6878.jpg","6878","/音频、视频、广播/6878.pdf","","6.35mm插头至RCA插孔","1.双极性单插头至单插孔；\r\n2.黑色手柄和银色设计便于使用。","插头","插孔","中心触点：镀镍黄铜","NA","NA","NA","NA","1000V"]
["899","音频、视频、广播","插头/插孔","/音频、视频、广播/6880.jpg","6880","/音频、视频、广播/6880.pdf","","RCA（耳机）插孔","1.RCA插孔和插头连接器；\r\n2.紧凑型设计；\r\n3.支持最大电缆外径为6.0 mm。","RCA（耳机）插孔","NA","阀体采用压铸锌合金；\r\n抗变色镀镍；\r\n触点为镀金黄铜","NA","NA","NA","NA","NA"]
["900","音频、视频、广播","插头/插孔","/音频、视频、广播/6881.jpg","6881","/音频、视频、广播/6881.pdf","","RCA（耳机）插头","1.RCA插孔和插头连接器；\r\n2.紧凑型设计；\r\n3.支持最大电缆外径为6.0 mm。","RCA（耳机）插头","NA","阀体采用压铸锌合金；\r\n抗变色镀镍；\r\n触点为镀金黄铜","NA","NA","NA","NA","NA"]
["901","音频、视频、广播","双香蕉插头","/音频、视频、广播/4044.jpg","4044","/音频、视频、广播/4044.pdf","","6.35mm（0.25in）耳机插孔至堆接双香蕉插头","1.允许双极性6.35mm(0.25in)插头与香蕉插孔或接线柱连接；\r\n2.阀体上的十字孔4.2mm(0.166in)可以提供侧堆叠连接。","6.35mm耳机插孔","双香蕉插头","耳机插孔：镀镍黄铜；\r\n绝缘:ABS模压到耳机插孔和香蕉插头；\r\n双香蕉插头：弹簧-镀镍铍铜\r\n阀体：镀镍黄铜","NA","NA","最高+ 50℃(+ 122℉)","NA","500V"]